Key notes: Shock controller must be in 8-pole scanned mode + remote + subject + high.

Verify prior that with set/test toggled and manual that it goes up to 1mA!